,Width##LENGTH##FEET,Weight Product##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Warranty Expiration##OTHER##,Voltage AC##OTHER##,Unbalanced Input Connector##OTHER##,Unbalanced Input Channels##OTHER##,URL##OTHER##,Type Image##OTHER##,Type Comments##OTHER##,Thermal Loss##HVAC_HEATING_LOAD##BRITISH_THERMAL_UNITS_PER_HOUR,Technology##OTHER##,THD+N##OTHER##,Subnet Mask##OTHER##,Signal to Noise (20Hz-20kHz @ 8Ω)##OTHER##,Serial Number##OTHER##,Sensitivity##OTHER##,Regulatory Compliance##OTHER##,Rack Units##OTHER##,Product Page URL##OTHER##,Product Documentation Link##OTHER##,Power Standby##OTHER##,Power Peak##OTHER##,Power Factor##OTHER##,Part Number##OTHER##,Panel Name##OTHER##,Operating Temperature Range##OTHER##,Number of Amplified Channels##OTHER##,Nominal Voltage##ELECTRICAL_POTENTIAL##VOLTS,Noise##OTHER##,Network Connections##OTHER##,Mounting##OTHER##,Mount Type##OTHER##,Model##OTHER##,Minimum Operating Voltage##ELECTRICAL_POTENTIAL##VOLTS,Maximum Output Voltage##ELECTRICAL_POTENTIAL##VOLTS,Maximum Output Power (per channel)##ELECTRICAL_WATTAGE##WATTS,Maximum Output Current (Peak)##ELECTRICAL_CURRENT##AMPERES,Maximum Operating Voltage##ELECTRICAL_POTENTIAL##VOLTS,Maximum Input Level##OTHER##,Market##OTHER##,Low Voltage Control##OTHER##,Line Level Outputs##OTHER##,Line Level Output Connectors##OTHER##,Install Date##OTHER##,Input Sensitivity##OTHER##,Input Impedance##OTHER##,IP Address##OTHER##,Housing Type##OTHER##,Height##LENGTH##FEET,Heat Load Standby##OTHER##,Heat Load Active##OTHER##,Gateway##OTHER##,Filter Maintenance##OTHER##,Fan Noise (Idle)##OTHER##,Manufacturer##OTHER##,Mains Voltage Connector##OTHER##,Enclosure##OTHER##,Double-Mounted##OTHER##,Digital Audio Output Channels##OTHER##,Digital Audio Input Channels##OTHER##,Description##OTHER##,Depth##LENGTH##FEET,Delay##OTHER##,Default Gain##OTHER##,Default Elevation##LENGTH##FEET,DSP Precision##OTHER##,DSP Latency##OTHER##,Current Draw##OTHER##,Crosstalk##OTHER##,Cost##CURRENCY##CURRENCY,Communication Ports##OTHER##,Communication Formats##OTHER##,Chassis Material##OTHER##,Centered##LENGTH##FEET,Breaker Requirement##ELECTRICAL_CURRENT##AMPERES,Bracket Material##OTHER##,Balanced Input Connectors##OTHER##,Balanced Input Channels##OTHER##,Assembly Code##OTHER##,Apparent Power (longterm)##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,Apparent Power (in-rush)##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,Amplified Outputs##OTHER##,Amplified Output Connectors##OTHER##,Air-Flow##OTHER##
Mezzo 322 A double-mounted,0.689127604167,5.73,73.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-322-a,mezzo322A_rear.png,(2) Channel Audio Amplifier w/ DSP,113.000000000000,Mezzo,0.00x %,,>103 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-322-a,https://www.powersoft-audio.com/en/docman/1444-powersoft-mezzo-ds-en-web/file,11,85,0.91,0613,Mezzo 322 A,14°F to 113°F,2,100.000000000000,30,1,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 322 A,90.000000000000,142.000000000000,160.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,2,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,38,113,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,1,0,0,(2) Channel Audio Amplifier w/ DSP,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,100Mbps,Galvanized Steel,0.698208051280,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,2,D5030100,80.400000000000,468.000000000000,2,EURO 5mm,Internally Cooled
Mezzo 322 AD single-mounted,0.689127604167,5.73,73.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-322-ad,mezzo322AD_rear.png,2-channel Audio Amplifier w/ DSP & Network Audio,116.000000000000,Mezzo,0.00x %,,>103 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-322-ad,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,11,86,0.91,0617,Mezzo 322 AD,14°F to 113°F,2,100.000000000000,30,2,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 322 AD,90.000000000000,142.000000000000,160.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,2,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,41,116,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,0,4,4,2-channel Audio Amplifier w/ DSP & Network Audio,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.343750000000,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,2,D5030100,80.400000000000,468.000000000000,2,EURO 5mm,Internally Cooled
Mezzo 324 A single-mounted,0.689127604167,5.73,76.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-324-a,mezzo324A_rear.png,(4) Channel Audio Amplifier w/ DSP,124.000000000000,Mezzo,0.00x %,,>100 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-324-a,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,15,89,0.89,0612,Mezzo 324 A,14°F to 113°F,4,100.000000000000,30,1,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 324 A,90.000000000000,142.000000000000,80.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,0,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,50,124,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,0,0,0,(4) Channel Audio Amplifier w/ DSP,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.343750000000,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,4,D5030100,85.200000000000,468.000000000000,4,EURO 5mm,Internally Cooled
Mezzo 324 AD single-mounted,0.689127604167,5.73,77.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-324-ad,mezzo322AD_rear.png,4-channel Audio Amplifier w/ DSP & Network Audio,127.000000000000,Mezzo,0.00x %,,>100 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,11,86,0.89,0316,Mezzo 324 AD,14°F to 113°F,4,100.000000000000,30,2,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 324 AD,90.000000000000,142.000000000000,80.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,0,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,54,127,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,0,4,4,4-channel Audio Amplifier w/ DSP & Network Audio,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.343750000000,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,4,D5030100,85.200000000000,468.000000000000,2,EURO 5mm,Internally Cooled
Mezzo 602 A single-mounted,0.689127604167,5.73,125.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-602-a,mezzo602A_rear.png,(2) Channel Audio Amplifier w/ DSP,169.000000000000,Mezzo,0.00x %,,>105 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-602-a,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,11,125,0.93,0611,Mezzo 602 A,14°F to 113°F,2,100.000000000000,30,1,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 602 A,90.000000000000,142.000000000000,300.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,2,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,37,169,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,0,0,0,(2) Channel Audio Amplifier w/ DSP,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.343750000000,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,2,D5030100,134.400000000000,468.000000000000,2,EURO 5mm,Front to Back
Mezzo 602 AD single-mount,0.689127604167,5.73,126.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-602-ad,mezzo602AD_rear.png,2-channel Audio Amplifier w/ DSP & Network Audio,172.000000000000,Mezzo,0.00x %,,>105 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-602-ad,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,12,101,0.93,0615,Mezzo 602 AD,14°F to 113°F,2,100.000000000000,30,2,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 602 AD,90.000000000000,142.000000000000,300.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,2,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,40,172,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,0,4,4,2-channel Audio Amplifier w/ DSP & Network Audio,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.343750000000,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,2,D5030100,135.600000000000,468.000000000000,2,EURO 5mm,Front to back
Mezzo 604 A single-mount,0.689127604167,5.73,129.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-604-a,mezzo604A_rear.png,(4) Channel Audio Amplifier w/ DSP,185.000000000000,Mezzo,0.00x %,,>100 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-604-a,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,15,150,0.93,0610,Mezzo 604 A,14°F to 113°F,2,100.000000000000,30,1,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 602 A,90.000000000000,142.000000000000,150.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,2,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,50,185,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,0,0,0,(4) Channel Audio Amplifier w/ DSP,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 DB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.343750000000,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,4,D5030100,139.200000000000,468.000000000000,4,EURO 5mm,Front to Back
Mezzo 604 AD_single-mount,0.689127604167,5.73,130.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-604-ad,mezzo604AD_rear.png (2),4-channel Audio Amplifier w/ DSP & Network Audio,188.000000000000,Mezzo,0.00x %,,>102 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-604-ad,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,11,151,0.93,0614,Mezzo 604 AD,14°F to 113°F,2,100.000000000000,30,2,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 604 AD,90.000000000000,142.000000000000,150.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,0,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,53,188,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,0,4,4,4-channel Audio Amplifier w/ DSP & Network Audio,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.343750000000,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,4,D5030100,140.400000000000,468.000000000000,4,EURO 5mm,Front to back
Mezzo 604 AD_double-mount,0.689127604167,5.73,130.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-604-ad,mezzo604AD_rear.png (2),4-channel Audio Amplifier w/ DSP & Network Audio,188.000000000000,Mezzo,0.00x %,,>102 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-604-ad,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,11,151,0.93,0614,Mezzo 604 AD,14°F to 113°F,2,100.000000000000,30,2,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 604 AD,90.000000000000,142.000000000000,150.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,0,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,53,188,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,1,4,4,4-channel Audio Amplifier w/ DSP & Network Audio,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.697916666667,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,4,D5030100,140.400000000000,468.000000000000,4,EURO 5mm,Front to back
Mezzo 604 A double-mount,0.689127604167,5.73,129.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-604-a,mezzo604A_rear.png,(4) Channel Audio Amplifier w/ DSP,185.000000000000,Mezzo,0.00x %,,>100 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-604-a,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,15,150,0.93,0610,Mezzo 604 A,14°F to 113°F,2,100.000000000000,30,1,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 602 A,90.000000000000,142.000000000000,150.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,2,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,50,185,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,1,0,0,(4) Channel Audio Amplifier w/ DSP,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 DB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.697916666667,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,4,D5030100,139.200000000000,468.000000000000,4,EURO 5mm,Front to Back
Mezzo 602 AD double-mount,0.689127604167,5.73,126.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-602-ad,mezzo602AD_rear.png,2-channel Audio Amplifier w/ DSP & Network Audio,172.000000000000,Mezzo,0.00x %,,>105 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-602-ad,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,12,101,0.93,0615,Mezzo 602 AD,14°F to 113°F,2,100.000000000000,30,2,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 602 AD,90.000000000000,142.000000000000,300.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,2,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,40,172,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,1,4,4,2-channel Audio Amplifier w/ DSP & Network Audio,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.697916666667,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,2,D5030100,135.600000000000,468.000000000000,2,EURO 5mm,Front to back
Mezzo 602 A double-mounted,0.689127604167,5.73,125.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-602-a,mezzo602A_rear.png,(2) Channel Audio Amplifier w/ DSP,169.000000000000,Mezzo,0.00x %,,>105 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-602-a,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,11,125,0.93,0611,Mezzo 602 A,14°F to 113°F,2,100.000000000000,30,1,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 602 A,90.000000000000,142.000000000000,300.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,2,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,37,169,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,1,0,0,(2) Channel Audio Amplifier w/ DSP,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.697916666667,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,2,D5030100,134.400000000000,468.000000000000,2,EURO 5mm,Front to Back
Mezzo 324 AD double-mounted,0.689127604167,5.73,77.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-324-ad,mezzo322AD_rear.png,4-channel Audio Amplifier w/ DSP & Network Audio,127.000000000000,Mezzo,0.00x %,,>100 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,11,86,0.89,0316,Mezzo 324 AD,14°F to 113°F,4,100.000000000000,30,2,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 324 AD,90.000000000000,142.000000000000,80.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,0,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,54,127,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,1,4,4,4-channel Audio Amplifier w/ DSP & Network Audio,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.697916666667,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,4,D5030100,85.200000000000,468.000000000000,2,EURO 5mm,Internally Cooled
Mezzo 324 A double-mounted,0.689127604167,5.73,76.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-324-a,mezzo324A_rear.png,(4) Channel Audio Amplifier w/ DSP,124.000000000000,Mezzo,0.00x %,,>100 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-324-a,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,15,89,0.89,0612,Mezzo 324 A,14°F to 113°F,4,100.000000000000,30,1,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 324 A,90.000000000000,142.000000000000,80.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,0,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,50,124,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,1,0,0,(4) Channel Audio Amplifier w/ DSP,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.697916666667,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,4,D5030100,85.200000000000,468.000000000000,4,EURO 5mm,Internally Cooled
Mezzo 322 AD double-mounted,0.689127604167,5.73,73.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-322-ad,mezzo322AD_rear.png,2-channel Audio Amplifier w/ DSP & Network Audio,116.000000000000,Mezzo,0.00x %,,>103 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-322-ad,https://www.powersoft.com/wp-content/uploads/2019/06/powersoft_Mezzo_DS_EN_WEB-1.pdf,11,86,0.91,0617,Mezzo 322 AD,14°F to 113°F,2,100.000000000000,30,2,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 322 AD,90.000000000000,142.000000000000,160.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,2,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,41,116,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,1,4,4,2-channel Audio Amplifier w/ DSP & Network Audio,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,1000BASE-T,Galvanized Steel,0.697916666667,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,2,D5030100,80.400000000000,468.000000000000,2,EURO 5mm,Internally Cooled
Mezzo 322 A single-mounted,0.689127604167,5.73,73.000000000000,,100-240 VAC @ 50-60Hz,3.5mm mini-jack,2,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-322-a,mezzo322A_rear.png,(2) Channel Audio Amplifier w/ DSP,113.000000000000,Mezzo,0.00x %,,>103 dB,,4,"CE, CSA",0.5,https://www.powersoft.com/en/products/install-amps/mezzo-series/mezzo-322-a,https://www.powersoft-audio.com/en/docman/1444-powersoft-mezzo-ds-en-web/file,11,85,0.91,0613,Mezzo 322 A,14°F to 113°F,2,100.000000000000,30,1,"Rack, Surface and Plenum Mounting","Rack, Surface and/or Plenum",Mezzo 322 A,90.000000000000,142.000000000000,160.000000000000,15.600000000000,264.000000000000,18 dBu,Install,1,2,EURO 3.8mm,,4 dBu (balanced) | -10 dBV (unbalanced),"10kΩ to GND, 20kΩ balanced",,Steel,0.130859375000,38,113,,,26 dBA,Powersoft,IEC 10A,Galvanized Steel,0,0,0,(2) Channel Audio Amplifier w/ DSP,0.902343750000,100 ms,35.2 dB,4.000000000000,32 bit,2.5 ms,3.84,-60 dB,0.000000000000,8P8C,100Mbps,Galvanized Steel,0.343750000000,4.000000000000,Painted Galvanized Steel,EURO 3.8mm,2,D5030100,80.400000000000,468.000000000000,2,EURO 5mm,Internally Cooled
