,Width##LENGTH##FEET,Weight Product##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Warranty Expiration##OTHER##,URL##OTHER##,Type Image##OTHER##,Type Comments##OTHER##,Technology##OTHER##,Serial Number##OTHER##,Regulatory Compliance##OTHER##,Product Page URL##OTHER##,Product Documentation Link##OTHER##,Power Peak##OTHER##,Power Handling##OTHER##,Peak Mass Displacement##LENGTH##FEET,Peak Force (1250 W)##OTHER##,Part Number##OTHER##,Nominal BI##OTHER##,Mount Type##OTHER##,Motor strength (Bl)²/Re##OTHER##,Model##OTHER##,Market##OTHER##,Manufacturer URL##OTHER##,Manufacturer##OTHER##,Magnet Weight##OTHER##,Magnet Type##OTHER##,Inductace @ 100 Hz##OTHER##,Impedance##OTHER##,Housing Type##OTHER##,Height##LENGTH##FEET,Frequency Response##OTHER##,Force Factor##OTHER##,Description##OTHER##,Depth##LENGTH##FEET,Default Elevation##LENGTH##FEET,DC Resistance##OTHER##,Cost##CURRENCY##CURRENCY,Communication Ports##OTHER##,Assembly Code##OTHER##
Mover 4 Ohm,0.294921875000,5.38,625.000000000000,,https://www.powersoft.com/en/products/transducers/mover/,Mover ID.png,Inertial Drive 4 Ω,Mover,,"CE, CSA",https://www.powersoft.com/en/products/transducers/mover/,https://www.powersoft.com/wp-content/uploads/2019/10/powersoft_Mover_DS_EN-1.pdf,1250,625,0.032552083333,200 lbf,0672,32 Tm,Surface,282 (TM)²/Ω,Mover 4 Ohm,Install,https://www.powersoft.com/en/,Powersoft,10 oz,Neodymium grade 50 MGOe,25.8 mH,4,Steel,0.294921875000,0 - 500 Hz,4.5 lbf/W,Transducer,0.294921875000,0.000000000000,3.6 Ω,0.000000000000,Metric #4 Screw Terminals,D5030100
Mover 16 Ohm,0.294921875000,5.38,625.000000000000,,https://www.powersoft.com/en/products/transducers/mover/,Mover ID.png,Inertial Drive 16 Ω,Mover,,"CE, CSA",https://www.powersoft.com/en/products/transducers/mover/,https://www.powersoft.com/wp-content/uploads/2019/10/powersoft_Mover_DS_EN-1.pdf,1250,625,0.032552083333,200 lbf,0673,52 Tm,Surface,282 (TM)²/Ω,Mover 16 Ohm,Install,https://www.powersoft.com/en/,Powersoft,10 oz,Neodymium grade 50 MGOe,25.8 mH,16,Steel,0.294921875000,0 - 500 Hz,4.5 lbf/W,Transducer,0.294921875000,0.000000000000,9.7 Ω,0.000000000000,Metric #4 Screw Terminals,D5030100
